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· 8-port 1000Mbps SFP
· 2-port 10/100/1000Mbps RJ45

 Industrial conformance
· 12V to 52V DC, redundant power input
· -40℃ to 80℃ operating temperature
· IP40 aluminum housing
· Supports 6KV DC Ethernet ESD protection
· Supports 6KV DC EFT protection for power line
· Free Fall, Shock and Vibration Stability
· DIN-rail design

Slim Type with more Practicability and Convenience
LBTD82G-SFP an hardened 10-port Industrial Ethernet Switch, provides non-blocking wire-speed performance in harsh industrial environment. It also provides 8-port 1000Mbps SFP+2G RJ45 copper interfaces delivered in an IP40 rugged, strong case with redundant power system. Its slim case is suitable for such applications as surveillance system deployments, control management and wireless service in climatically demanding environments with wide temperature range from -40℃ to 80℃.

The LBTD82G-SFP  series is packaged in a compact IP40 case with Din-rail installation. It provides an integrated power supply with a wide range of voltages for worldwide operation. It also offers dual-redundant, reversible polarity 12V DC to 52V DC power supply inputs for high availability applications requiring dual or backup power inputs.






Specifications:
	Model No.
	LBTD82G-SFP 

	Ports
	8 port SFP support gigabit
2 port RJ45 10/100/1000Mbps

	
Performance Specification
	Bandwidth: 20Gbps 
Packet Buffer Memory:2Mbit
Packet Forwarding Rate:15Mpps
MAC Address Table: 8K

	Installation
	DIN rail

	Maximum Frame Size
	9000bytes packet size

	Flow Control
	Back pressure for half duplex, IEEE 802.3x pause frame for full duplex

	Enclosure
	IP40 aluminum housing

	
LED Indicator
	Power: Red
Copper / SFP : Link / Act 

	Power Input
	12 to 52V DC redundant power 

	Power Consumption
	< 10 watts

	Surge protection
	±4KV 

	
Network Protocols
	IEEE802.3 10BASE-T; 
IEEE802.3i 10Base-T; 
IEEE802.3u;100Base-TX; 
IEEE802.3ab 1000Base-T;  
IEEE802.3z 1000Base-X; 
IEEE802.3x;

	Network cables
	10BASE-T: Cat3,4,5 UTP(≤100 meter)     
100BASE-TX: Cat5 or later UTP(≤100meter)
1000BASE-TX: Cat6 or later UTP(≤100 meter)

	

Industry Standard
	FCC CFR47 Part 15,EN55022/CISPR22, Class A 
IEC61000-4-2 (ESD): ±8kV (contact), ±12kV (air)
IEC61000-4-3 (RS): 10V/m (80~1000MHz)
IEC61000-4-4 (EFT): Power Port: ±4kV; Data Port: ±2kV
IEC61000-4-5 (Surge): Power Port: ±2kV/DM, ±4kV/CM; Data Port: ±2kV
IEC61000-4-6 (CS): 3V (10kHz-150kHz); 10V (150kHz-80MHz)
IEC61000-4-16 (Common mode conduction): 30V (cont.), 300V (1s)

	Certification
	CE FCC Rohs compliance

	MTBF
	>300,000hours

	Dimensions (W x D x H)
	143.7×125×47.7mm 

	Weight
	Product Weight: 0.85KG
Packing Weight:1.0 KG

	Working Environment

	Working temperature: -40-80 degree  
Storage temperature: -40-80 degree
Relative Humidity: 5%~95 %( no condensation)

	Warranty 
	1-year replacement with new item; 3-years for main parts.  
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