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LBT248GST4-SFP 
[bookmark: OLE_LINK2]24-Port gigabit SFP +8G RJ45 combo+4-Port 10G SFP 
L3 Managed Industrial Switch  
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Rack mounted Aluminum Industrial SwitchFeatures
· Data control: support 802.3x full duplex flow control, support network storm suppression
· Redundant network: support STP/RSTP/MSTP, support ERPS (self-healing time <20ms)
· Support IPv6, static routing, Dynamic routing (RIP,OSPF)
· Support RIPng, OSPFv3, DHCP Server, DHCP replay, Qos
· Multicast management: Support IGMP Snooping V1/V2/V3
· VLAN: support IEEE 802.1q VLAN, effectively isolated broadcast domain
· Link aggregation: support link static/dynamic aggregation, provide perfect bandwidth utilization
· QoS: Support COS\DSCP, 4 queues, support WRR\SP scheduling mode
· Security management: support ACL access control list, support 802.1x, support user classification management
·  Management function: support Web, SNMP management mode
· Monitoring maintenance: support port mirroring, interface status monitoring, log management
· Alarm function: support power supply, port, abnormal state relay output





[bookmark: _GoBack]LBT248GST4-SFP switch is a high performance 10G SFP+ L3 core switch. It provides Static routing and dynamic routing with advanced hardware processing capacity. The machine adopts modular design, which supports up to 4 Port 10G SFP+, and retains the expansion ability to further support 10GE when realizing gigabit convergence or access. It supports IPv4/IPv6 hardware double stack and line speed forwarding, so that customers can easily cope with the coming IPv6 era, which provides high capacity exchange capacity. LBT248GST4-SFP switch has the operating temperature of -40℃ ~ 85℃, has the super firmness to adapt to all kinds of harsh environment, can also be very convenient to install in the machine room cabinet. The rack-mounted characteristics and wide temperature operation make the switch a plug and play industrial-grade device, providing a reliable and convenient solution for users to network their Ethernet devices.


Strong processing ability
LBT248GST4-SFP switch is based on the powerful and stable
processing power of VCore-III MIPS-based CPU
LBT248GST4-SFP provides up to 598Gbps of switching capacity
port full speed filtering and forwarding 252Mpps
To ensure that the trunk network of large traffic data without blocking
Forwarding.





Specifications:ROBOT
ROBOT

	Model No.
	LBT248GST4-SFP

	Interface
	24-Port 10/100/1000Mbps SFP 
8-Port 10/100/1000Mbps RJ45 (combo)
4-Port 10G SFP+
1-Port console

	
Performance Specification
	Bandwidth(switch capacity): 598Gbps 
Packet Buffer Memory:32Mbit
Packet Forwarding Rate: 252Mpps
MAC Address Table: 32K

	Installation
	Bracket mounted

	Maximum Frame Size
	16360bytes

	Flow Control
	Back pressure for half duplex, IEEE 802.3x pause frame for full duplex

	Enclosure
	IP50 Aluminum housing

	
LED Indicator
	Power: Red
Fiber: Link 2(Green)
Ethernet: Yellow 

	Dual Power Input
	36 to 72V DC &110～240V/50～60Hz AC

	Power Consumption
	< 45watts

	Surge protection
	±4KV 

	
Network Protocols
	IEEE802.3 10BASE-T; 
IEEE802.3i 10Base-T; 
IEEE802.3u;100Base-TX/FX; 
IEEE802.3ab 1000Base-T;  
IEEE802.3z 1000Base-X; 
IEEE802.3x;

	Network cables
	10BASE-T: Cat3,4,5 UTP(≤100 meter)     
100BASE-TX: Cat5 or later UTP(≤10meter)
1000BASE-TX: Cat6 or later UTP(≤100 meter)

	

Industry Standard
(EMC 4)
	FCC CFR47 Part 15,EN55022/CISPR22, Class A 
IEC61000-4-2 (ESD): ±8kV (contact), ±12kV (air)
IEC61000-4-3 (RS): 10V/m (80~1000MHz)
IEC61000-4-4 (EFT): Power Port: ±4kV; Data Port: ±2kV
IEC61000-4-5 (Surge): Power Port: ±2kV/DM, ±4kV/CM; Data Port: ±2kV
IEC61000-4-6 (CS): 3V (10kHz-150kHz); 10V (150kHz-80MHz)
IEC61000-4-16 (Common mode conduction): 30V (cont.), 300V (1s)

	Certification
	CE FCC Rohs compliance

	MTBF
	>300,000hours

	Dimensions (W x D x H)
	442×325×44mm

	Weight
	Product Weight: 4KGS    
Packing Weight: 4.15KGS

	Working Environment

	Working temperature: -40～85℃ ;  
Storage temperature: -40～85℃
Relative Humidity: 5%~95 %( no condensation)

	Warranty 
	1-year replacement with new item; 3-years for main parts.  













Dimensions
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Ordering Information
	LBT248GST4-SFP
	24-Port gigabit SFP +8G RJ45 combo+4-Port 10G SFP L3 Managed Industrial Switch
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